# -*- coding: utf-8 -*-

{
    'en':
    {
        # atDebug.py

        u'AT指令调试': 'AT debug',
        u'进入指令模式': 'Command mode',
        u'发送当前行的AT指令': 'Send Command line',
        u'+++\n#查询版本号\nAT+VERS\nAT+CSQ\nAT+CREG?\n': '+++\n#Query version\nAT+VERS\nAT+CSQ\nAT+CREG?\n',

        # atGroupBox.py

        u'除': 'Divide',
        u'恢复默认设置  ': 'Default settings  ',
        u'当前配置保存指令: ': 'Save command for the settings: ',
        u'参数索引:': 'Parameter index:',
        u'读取': 'Read',
        u'写入': 'Write',
        u'索引': 'Index',
        u'先读后写': 'Read ahead',
        u'发送': 'Send',
        u'先读后发': 'Read ahead',

        # configStore.py

        u'所有配置项': 'Load && save configuration',
        u'导入预存配置 -> 当前配置 (不保存)  ': 'Import configuration',
        u'导入预存配置 -> 新预存配置(保存并载入)  ': 'Import configuration to stored and load',
        u'导出预存配置  ': 'Export stored configuration  ',
        u'预存配置名:': 'Stored:',
        u'从设备读取': 'Load from device',
        u'保存到设备': 'Save to device',
        u'从预存配置读取': 'Load from stored',
        u'保存到预存配置': 'Save to stored',
        u'查看当前配置': 'List config',
        u'自定义附加指令:': 'Append AT commands',
        u'默认': 'Default',
        u'删除预存配置': 'Delete stored configuration',
        u'是否删除预存配置: ': 'Delete stored configuration: ',
        u'当前无连接设备': 'No connected device',
        u'预存配置: ': 'Stored configuration: ',
        u' 读取': ' read',
        u'成功': ' success',
        u'失败': ' failed',
        u'保存预存配置': 'Store configuration',
        u'是否保存当前配置到预存配置: ': 'Store configuration: ',
        u' 保存': ' save ',
        u'导入预存配置': 'Import configuration',
        u'读取文件 ': 'Read file ',
        u' 失败': ' failed',
        u'导入预存配置 ': 'Import configuration ',
        u'导入的预存配置所属产品与当前产品不一致': 'The Imported configuration is not fit the device',
        u'导入配置失败: ': 'Import configuration failure: ',
        u'导入配置: ': 'Import configuration: ',
        u'导出预存配置': 'Export stored configuration',
        u' 导出成功 ': ' export success',
        u' 导出失败': ' export failed',

        # connectSetup.py

        u'设备连接设置': 'Device connection settings',
        u'连接参数:': 'Connection:',
        u'刷新': 'Reflash',
        u'波特率:': 'Baud:',
        u'数据位:': 'Data:',
        u'停止位:': 'Stop:',
        u'校验位:': 'Parity:',
        u'0: 无': '0: None',
        u'1: 奇': '1: Odd',
        u'2: 偶': '2: Even',
        u'3: 空': '3: Space',
        u'连接设备': 'Connect',
        u'断开设备连接': 'Disconnect',
        u'配置模式连接': 'Config mode',

        # updateCheck.py

        u'应用程序升级检测': 'Upgrade detection',
        u'自动升级检测': 'Auto upgrade detection',
        u'当前版本:': 'Version:',
        u'升级检测': 'Detect',
        u'配置软件版本检测': 'Upgrade detection',

        # options.py

        u'其它选项': 'Other options',
        u'强制变更扩展程序': 'Force download extension',

        # update_handler.py

        u'连接升级服务器失败, 请稍后重试': 'Failed to connect to upgrade server. Please try again later',
        u'最新版本: ': 'Latest version: ',
        u'删除文件失败, 请关闭程序后重试': 'Failed to delete the files. Please close the program and try again',
        u'复制文件失败, 请关闭程序后重试': 'Failed to copy the files. Please close the program and try again',
        u'开始下载升级文件': 'Start downloading upgrade files',
        u'下载升级文件失败, 请稍后重试': 'Failed to download upgrade file. Please try again later',
        u'升级文件解压测试错误, 请稍后重试': 'Failed to unzip upgrade file. Please try again later',
        u'下载升级文件 %s 成功': 'Download upgrade file %s succeeded',
        u'关闭程序后等待新程序自动重启': 'Close the program and wait for the new program to restart automatically',

        # dtu4G_config.py

        u' 文件下载失败': ' file download failed',
        u'下载扩展程序\r\n': 'Download extension\r\n',
        u'下载文件: ': 'Download file: ',
        u'文件打开失败': 'Open file failed',
        u' 设备连接失败': ' failed to connect device',
        u' 设备连接成功': ' device connected successfully',
        u' 设备连接中...': ' device connection in progress...',
        u' 端口连接中...': ' connection in progress',
        u' 端口打开成功': ' connect successfully',
        u'等待设备上电进入配置模式': 'Wait for the device to power on and enter the configuration mode',
        u' 设备重连成功': ' device reconnected successfully',
        u' 设备重连中...': ' device reconnection in progress...',
        u' 端口打开失败': ' com open failed',
        u' 关闭端口中 ...': ' com close in progress ...',
        u' 端口已关闭': ' com closed',
        u'共发送指令: %d, 失败: %d\r\n': 'Total commands sent: %d, failed: %d\r\n',
        u'\r\n设备关闭连接\r\n': '\r\nDevice closed the connection\r\n',
        u'\r\n等待设备进入配置模式超时\r\n': '\r\nTimeout waiting for device to enter the configuration mode',

        # main_window.py

        u'读取当前页配置  ': 'Read all configuration of the page  ',
        u'扩展程序检测': 'Extension check',
        u'需要向设备安装或更新扩展程序才可完成所有AT指令设置\n是否安装最新扩展程序？': 'The device should install or update extension to perform all configuration\nDo you want to install the latest extension?',
        u'当前产品选项不支持此扩展程序，请选择正确产品选项或联系客服！': 'The extension is not fit the device, please select the correct product in menu or contact customer service',
        u'主程序检测': 'Firmware check',
        u'当前产品选项不支持此产品，请选择正确产品选项或联系客服！': 'The selected product option does not support this device. Please select the correct product option or contact customer service!',
        u'程序升级检测': 'Upgrate check',
        u'确认是否下载并升级到最新版本': 'Confirm whether to download and upgrade to the latest version',
        u'主控面板': 'Main control panel',
        u'当前产品系列：': 'Current series: ',
        u'选择产品系列': 'Select product series',

        # default_at_description.py

        u'保存配置': 'Save DTU configuration',
        u'版本': 'Version',
        u'主程序版本': 'Firmware',
        u'扩展程序版本': 'Extension',
        u'设备编号': 'Device ID',
        u'应用编号': 'Application ID',
        u'启动信息': 'Startup string',
        u'主服务器连接方式': 'Main server connection mode',
        u'连接方式': 'Connection mode',
        u': 被动单次模式': ': Manual',
        u': 主动常连模式': ': Constant',
        u'主服务器': 'Main server url',
        u'服务器url': 'Server url',
        u'主服务器报文模式': 'Protocol for main server transmission',
        u'报文模式': 'Protocol',
        u'主服务器上传心跳': 'Upload heart data for main server',
        u'心跳间隔': 'Heart interval',
        u' 秒': ' seconds',
        u'心跳数据': 'Heart data',
        u'自定义注册包': 'Customize registration package',
        u'注册包': 'Registration',
        u'主服务器下传数据最大时间间隔': 'Timeout to reset connection when no download data from main server',
        u'时间间隔': 'Interval',
        u'网口配置': 'Lan configuration',
        u'IP地址': 'IP address',
        u'子网掩码': 'Subnet mask',
        u'MAC地址': 'MAC address',
        u'DNS地址': 'DNS address',
        u'备份服务器': 'Standby server',
        u'并行服务器配置': 'Parallel server configuration',
        u'服务器心跳': 'Server heart',
        u'常在线': 'Always online',
        u': 否': ': NO',
        u': 是': ': YES',
        u'UDP模式': 'UDP protocol',
        u'不上传数据': 'Upload UART data',
        u'不下发数据': 'Out server data',
        u'SSL模式': 'SSL protocol',
        u'重启模式': 'Auto reboot mode',
        u'无SIM卡重启': 'Without SIM',
        u' 分钟': ' minutes',
        u'定间隔重启': 'Fixed interval',
        u'串口波特率': 'UART port baudrate',
        u'波特率': 'Baudrate',
        u'串口配置 ': 'UART port setting ',
        u'串口配置': 'setting',
        u'数据位': 'Data',
        u'停止位': 'Stop',
        u': 1个停止位': ': 1 stop bit',
        u': 2个停止位': ': 2 stop bits',
        u': 1.5个停止位': ': 1.5 stop bits',
        u'校验位': 'Parity',
        u': 无校验': ': None',
        u': 奇校验': ': Odd',
        u': 偶校验': ': Even',
        u': 空校验': ': Space',
        u'DTU启动执行AT指令': 'AT command Executed after bootup',
        u'AT指令': 'AT command',
        u'是否输出接收的短信内容': 'Indicate received SMS',
        u'是否输出': 'Indicate',
        u'控制短信号码过滤': 'Enable AT command SMS filter by phone number',
        u'是否过滤': 'Enable',
        u'控制短信有效号码': 'Phone number filter',
        u'有效号码': 'Phone number',
        u'是否启用扩展程序': 'Enable extension program',
        u'是否启用': 'Enable',
        u'本地端口绑定': 'Local socket bind port',
        u'绑定端口': 'Bind port',
        u'主服务器UDP连接': 'Main server transmission Using UDP protocol',
        u'是否UDP': 'Using UDP',
        u'DTU电话号码': 'DTU phone number',
        u'电话号码': 'Phone number',
        u'定间隔或定时任务': 'Fix interval or scheduled tasks',
        u'任务类型': 'Task type',
        u': 关闭任务': ': Close task',
        u': 定时输出文本': ': Scheduled output text',
        u': 定间隔输出文本': ': Fix interval output text',
        u': 定时执行at指令': ': Scheduled execute AT command',
        u': 定间隔执行at指令': ': Fix interval execute AT command',
        u': 定时执行at指令并且把结果用短信发送到指定的电话号码': ': Scheduled execute AT command and send respond SMS to a phone',
        u': 定间隔执行at指令并且把结果用短信发送到指定的电话号码': ': Fix interval execute AT command and send respond SMS to a phone',
        u'时间hhmm': 'Time(hhmm)',
        u'文本或AT指令': 'Text or AT',
        u'VPN网络配置': 'VPN configuration',
        u'VPN服务器url': 'VPN server url',
        u'网络名': 'Network name',
        u'网络密码': 'Network password',
        u'网络IP': 'VPN IP',
        u'网络MASK': 'VPN MASK',
        u'网络MTU': 'VPN MTU',
        u'运营商APN配置': 'The access point name configuration',
        u'运营商APN': 'APN',
        u'用户名': 'Username',
        u'密码': 'Password',
        u'认证模式': 'Authentication',
        u'外网端口访问黑名单': 'Internet port access blacklist',
        u'端口类型': 'port type',
        u': 关闭': ': Close',
        u'端口号': 'Port number',
        u'外网端口访问白名单': 'Internet port access whitelist',
        u'网络设备IP信息': 'Network interface IP',
        u': LAN口': ': LAN',
        u': 4G模块网口': ': 4G module',
        u': VPN网口': ': VPN interface',
        u': PPTP网口': ': PPTP interface',
        u': WIFI热点': ': WIFI AP interface',
        u': WIFI设备': ': WIFI client',
        u': USB网口': ': USB network interface',
        u'默认网关': 'Default gateway',
        u'网关IP': 'Gateway IP',
        u'PPTP VPN配置': 'PPTP VPN configuration',
        u'接入点域名': 'Dial in domain',
        u'网络定义': 'Netword define',
        u'是否开启mppe': 'Enable mppe',
        u'是否默认网关': 'As gateway',
        u'最大报文长度': 'Maximum package length',
        u'报文长度': 'Package length',
        u'串口数据包最小间隔时间': 'Minimum interval between UART port data package',
        u'间隔时间': 'Interval',
        u' 毫秒': ' millisecond',
        u'移动模块工作模式': 'DTU Work mode',
        u'工作模式': 'Work mode',
        u': 数据模式': ': Internet access mode',
        u': 短信模式': ': No internet mode',
        u': VPN路由模式': ': VPN router mode',
        u'虚拟端口映射，TCP/UDP数据转发': 'Virtual NAT, TCP/UDP data forward',
        u': TCP模式': ': TCP',
        u': UDP模式': ': UDP',
        u'源端口号': 'Source port',
        u'目标ip:端口': 'Target IP:port',
        u'端口映射配置，IP包转发，局域网设备需要设置DTU为网关': 'PORT MAPPING, IP packet forward, LAN devices need to set DTU as gateway',
        u'WIFI总开关': 'WIFI main switch',
        u'是否关闭': 'Switch',
        u': 关闭wifi设备': ': WIFI disable',
        u': 打开wifi设备': ': WIFI enable',
        u'不设置': 'Not set',
        u'通道号': 'Channel number',
        u'WIFI热点参数': 'WIFI AP configuration',
        u'热点名': 'AP name',
        u'加密方式': 'Encryption',
        u': 不加密': ': None',
        u': psk2加密': ': PSK2 encryption',
        u'WIFI热点DHCP开关': 'DHCP service for WIFI AP',
        u'DHCP开关': 'DHCP',
        u': 关闭DHCP服务': ': Disable DHCP service',
        u': 开启DHCP服务': ': enable DHCP service',
        u'DHCP配置': 'DHCP configuration',
        u'起始偏移数': 'Start count',
        u'总个数': 'Limit count',
        u'WIFI终端配置': 'WIFI client configuration',
        u'WIFI终端开关': 'WIFI client',
        u': 关闭WIFI终端': ': Disable',
        u': 开启WIFI终端': ': Enable',
        u'加密模式': 'Encryption',
        u'WIFI终端IP配置': 'WIFI client IP configuration',
        u'IP模式': 'IP mode',
        u': 动态获取': ': DHCP',
        u': 静态设置': ': STATIC',
        u'静态IP地址': 'Static ip address',
        u'WIFI配置立刻生效': 'Reload all WIFI configuration',
        u'列出WIFI热点': 'WIFI AP List',
        u'串口数据模式下是否输出主服务器连接状态': 'Whether to indicate the connection status of the main server to UART',
        u'是否启动网管服务': 'Management service on network',
        u'是否启动': 'The function',
        u': 不启动': ': Disable',
        u': 启动': ': Enable',
        u'DTU软件重启': 'DTU software restart',
        u'DTU重启方式': 'DTU reboot type',
        u'重启类型': 'Reboot type',
        u': DTU软件重启': ': DTU software restart',
        u': 软重启': ': Reboot',
        u': 硬重启': ': Repower',
        u': 仅4G模块重启': ': 4G module reboot',
        u'IMEI号': 'IMEI',
        u'WIFI终端静态IP配置下的网关': 'WIFI client default gateway configuration in static IP mode',
        u'联网自动切换设置': 'Internet connection automode setting',
        u'联网模式': 'Internet mode',
        u': 关闭自动切换': ': No automode',
        u': WIFI优先': ': WIFI priority',
        u': 4G优先': ': 4G priority',

        # products\product_dtu4G_common\at_description.conf


        # products\product_dtu4G_common\product.conf

        u'4G DTU 通用配置': '4G DTU configuration',
        u'DTU 通用配置': 'DTU configuration',
        u'版本和编号': 'Verison & ID',
        u'高级选项': 'Advanced setting',
        u'串口通讯主服务器配置': 'Socket & serial setting',
        u'多服务器配置': 'Multi-servers setting',
        u'网口通讯配置': 'Network setting',
        u'短信配置': 'SMS setting',
        u'WIFI设置': 'WIFI setting',
        u'保存&重启': 'Save & Reboot',

        # products\product_dtu4G_io_report\at_description.conf

        u'管脚别名，在短信报警中使用': 'Pin alias, used in SMS alarm',
        u'管脚号': 'Pin number',
        u'别名': 'Alias',
        u'短信报警号码': 'SMS alarm phone number',
        u'报警号码': 'Phone number',
        u'短信报警号码1': 'SMS alarm phone number1',
        u'短信报警号码2': 'SMS alarm phone number2',
        u'短信报警号码3': 'SMS alarm phone number3',
        u'短信报警号码4': 'SMS alarm phone number4',
        u'不同报警类型的在报警短信中报警内容': 'Alarm contents in each alarm type',
        u'报警类型': 'Alarm type',
        u': 低电平': ': Low level',
        u': 高电平': ': High level',
        u'报警内容': 'Alarm contents',
        u': 短息报警或字符串上传工作模式，由是否设置短信报警号码决定': ': SMS alarm or string upload, depends on SMS alarm number setting',
        u': 远程MODBUS工作模式': ': Remote MODBUS',
        u'本机MODBUS地址': 'Local MODBUS address',
        u'MODBUS地址': 'MODBUS address',
        u'字符串上传模式下，上报时间间隔': 'Interval in string upload working mode',
        u'保存4DI REPORT配置': 'Save 4DI REPORT configuration',
        u'管脚当前报警状态': 'Current alarm information for pins',
        u'管脚0报警状态': 'Pin0 alarm',
        u': 低电平报警': ': Low level alarm',
        u': 高电平报警': ': High level alarm',
        u': 未报警': ': No alarm',
        u'管脚1报警状态': 'Pin1 alarm',
        u'管脚2报警状态': 'Pin2 alarm',
        u'管脚3报警状态': 'Pin3 alarm',
		u'管脚报警类型配置': 'Pin Alarm Type Config',
		u'报警短信内容配置': 'Alarm SMS Content Config',
		u'接收报警短信号码': 'Received Alarm SMS phone',
		u'管脚保护时间': 'Pin protection time',
        u'保护时间': 'Protection time',
		u'语音拨号播放': 'Voice dialing playback',
		u'索引号': 'Index number',
		
        # products\product_dtu4G_io_report\product.conf

        u'DTU-4DI设置': 'DTU-4DI',
        u'4DI REPORT配置': '4DI REPORT setting',
		
		# products\product_dtu4G_4di_io_report\at_description.conf

        u'管脚别名，在短信报警中使用': 'Pin alias, used in SMS alarm',
        u'管脚号': 'Pin number',
        u'别名': 'Alias',
        u'短信报警号码': 'SMS alarm phone number',
        u'报警号码': 'Phone number',
        u'短信报警号码1': 'SMS alarm phone number1',
        u'短信报警号码2': 'SMS alarm phone number2',
        u'短信报警号码3': 'SMS alarm phone number3',
        u'短信报警号码4': 'SMS alarm phone number4',
        u'不同报警类型的在报警短信中报警内容': 'Alarm contents in each alarm type',
        u'报警类型': 'Alarm type',
        u': 低电平': ': Low level',
        u': 高电平': ': High level',
        u'报警内容': 'Alarm contents',
        u': 短息报警或字符串上传工作模式，由是否设置短信报警号码决定': ': SMS alarm or string upload, depends on SMS alarm number setting',
        u': 远程MODBUS工作模式': ': Remote MODBUS',
        u'本机MODBUS地址': 'Local MODBUS address',
        u'MODBUS地址': 'MODBUS address',
        u'字符串上传模式下，上报时间间隔': 'Interval in string upload working mode',
        u'保存4DI REPORT配置': 'Save 4DI REPORT configuration',
        u'管脚当前报警状态': 'Current alarm information for pins',
        u'管脚0报警状态': 'Pin0 alarm',
        u': 低电平报警': ': Low level alarm',
        u': 高电平报警': ': High level alarm',
        u': 未报警': ': No alarm',
        u'管脚1报警状态': 'Pin1 alarm',
        u'管脚2报警状态': 'Pin2 alarm',
        u'管脚3报警状态': 'Pin3 alarm',
		u'管脚配置': 'Pin config',
        u'低电平报警内容': 'Low alarm content',
        u'高电平报警内容': 'High alarm content',
		u'重复报警时间间隔': 'Interval for repeat alarm',
        u'管脚保护时间': 'Pin protection time',
        u'保护时间': 'Protection time',

        # products\product_dtu4G_4di_io_report\product.conf

        u'DTU-4DI-IO设置': 'DTU-4DI-IO',
        u'4DI REPORT配置': '4DI REPORT setting',


        # products\product_dtu4G_modbus_rtu2tcp\at_description.conf

        u'设备收到MODBUS RTU指令转换到MODBUS TCP指令': 'Convert MODBUS RTU instruction to Modbus TCP instruction',
        u'RTU设备ID': 'RTU device ID',
        u'TCP设备ID': 'TCP device ID',
        u'ip地址': 'IP address',
        u'RTU设备地址': 'RTU device ID',
        u'TCP设备地址': 'TCP device ID',

        # products\product_dtu4G_modbus_rtu2tcp\product.conf

        u'MODBUS_RTU2TCP配置': 'MODBUS_RTU2TCP setting',

        # products\product_dtu4G_modbus_tcp2rtu\at_description.conf

        u'设备收到MODBUS TCP指令转换到MODBUS RTU指令，如果RTU地址为0，则不做地址转换': 'Convert MODBUS TCP instruction to Modbus RTU instruction',

        # products\product_dtu4G_modbus_tcp2rtu\product.conf

        u'MODBUS_TCP2RTU配置': 'MODBUS_TCP2RTU setting',

        # products\product_dtu4G_mqttclient\at_description.conf

        u'MQTT用户名': 'MQTT user name',
        u'MQTT密码': 'MQTT password',
        u'MQTT发布主题': 'MQTT publish topic',
        u'发布主题': 'Publish topic',
        u'MQTT订阅主题': 'MQTT subscribe topic',
        u'订阅主题': 'Subscribe topic',
        u'MQTT客户端ID': 'MQTT client ID',
        u'客户端ID': 'client ID',
        u'MQTT客户端ID，默认空使用随机数避免ID冲突': 'MQTT client ID, empty by default to use random numbers to avoid ID conflicts',

        # products\product_dtu4G_mqttclient\product.conf

        u'4G DTU MQTT设置': '4G DTU MQTT',
        u'DTU-MQTT设置': 'DTU-MQTT',
        u'MQTT配置': 'MQTT setting',

        # products\product_dtu4G_NMEA0183_gps\at_description.conf

        u'网络摄像头rtsp链接': 'Webcam rtsp url',
        u'rtsp链接': 'Rtsp url',
        u'COMWAY协议上传图片，主服务器必须设置为COMWAY模式': 'Upload picture by main server COMWAY Packet format',
        u'是否使能': 'Enable',
        u'开始拍照': 'Take picture',
        u'GPS信息': 'GPS information',
        u'定位状态': 'Location status',
        u': 已定位': ': Available',
        u': 未定位': ': Invalid',
        u'纬度半球': 'Lat hemisphere',
        u'纬度': 'Latitudinal',
        u'格式ddmm.mmmm': 'Format(ddmm.mmmm)',
        u'经度半球': 'Long hemisphere',
        u'经度': 'longitude',
        u'格式dddmm.mmmm': 'Format(dddmm.mmmm)',
        u'速率标识': 'Speed flag',
        u'地面速率节': 'Speed(knot)',
        u'高度标识': 'Altitude flag',
        u'海拔高度': 'Altitude',
        u'GPS参数配置': 'GPS packet configuration',
        u': ID头固定域长模式': ': Head field fill with fix length ID',
        u': ID域为字符串模式': ': Head field fill with ID string',
        u': AT指令读取模式': ': GPS information read by AT command',
        u': ID域为字符串模，附加时间标签模式': ': Head field fill with ID string and time stamp',
        u': JSON格式': ': JSON format',
        u': COMWAY格式上传，主服务器必须设置为COMWAY模式': ': Main server COMWAY Packet format',
        u'上传GPS间隔': 'Upload cycle',
        u'速度阀值': 'Speed',
        u' 节×10': ' knot*10',
        u'低于阀值': 'Below',
        u'高于阀值': 'Above',
        u'保存数据': 'Store enable',
        u'JSON前缀是否加data=': 'Prefix data= in JSON format',
        u'GPS数据上传HTTP协议配置': 'Upload GPS packet by HTTP',
        u'服务器地址': 'Server domain',
        u'服务器端口': 'Server port',
        u'ssl连接': 'Ssl enbale',
        u'post路径': 'post path',
        u'post名称': 'post name',
        u'post文件名': 'post file name',
        u'MQTT服务器url': 'MQTT server url',
        u'MQTT服务器url，默认空用COMWAY方式连接mqtt.comway.com.cn:2883': 'MQTT server url, empty by default to connect mqtt.comway.com.cn:2883 by COMWAY mode',

        # products\product_dtu4G_NMEA0183_gps\product.conf

        u'4G DTU GPS设置': '4G DTU GPS',
        u'DTU-GPS设置': 'DTU-GPS',
        u'GPS和拍照配置': 'GPS or photograph setting',

        # products\product_dtu4G_take_picture\at_description.conf

        u'USB摄像头拍照配置': 'USBcam configuration',
        u'宽': 'Wide',
        u'高': 'High',
        u'延时': 'Delay',
        u'图片上传HTTP协议配置': 'Upload picture by HTTP',
        u'COMWAY协议上传图片使能': 'Upload picture by main server COMWAY Packet format',

        # products\product_dtu4G_take_picture\product.conf

        u'4G DTU 拍照功能设置': '4G DTU photograph',
        u'DTU-拍照设置': 'DTU-PHOTOGRAPH',
        u'拍照配置': 'photograph setting',

        # products\product_rtu716\at_description.conf

        u'RTU管脚配置': 'RTU pins configuration',
        u'管脚类型': 'Type of pin',
        u': 无效管脚': ': Invalid pin',
        u': 单端电压管脚': ': Single ended voltage',
        u': 单端电流管脚': ': Single ended current',
        u': LOGIC输入管脚': ': LOGIC input',
        u': LOGIC输出管脚': ': LOGIC output',
        u': 不报警': ': No alarm',
        u': 过压或过流报警': ': Overvoltage or overcurrent alarm',
        u': 欠压或欠流报警': ': Undervoltage or undercurrent alarm',
        u': 过压欠压或过流欠流都报警': ': Over or under alarm',
        u': 电平变化报警': ': LOGIC change alarm',
        u'上限值': 'Upper threshold',
        u'下限值': 'Lower threshold',
        u'逻辑输入反转': 'LOGIC reverse',
        u'逻辑输出初值': 'Output initial',
        u': 三态': ': Tristate',
        u'外部MODBUS设备读取指令': 'MODBUS device read instruction',
        u'MODBUS指令': 'Instruction',
        u'指令': 'Command',
        u': 读取': ': Read',
        u': 延时': ': Delay',
        u': 无': ': None',
        u'地址': 'Address',
        u'个数': 'Count',
        u'外部MODBUS设备串口配置': 'MODBUS device UART configuration',
        u'RTU采样参数': 'RTU configuration',
        u'采样时间间隔': 'Acquisition cycle',
        u'上报时间间隔': 'Reporting cycle',
        u'保存时间间隔': 'Store cycle',
        u'是否省电模式': 'Power mode',
        u': 正常模式': ': Normal power',
        u': 省电模式': ': Low power',
        u'读取最新记录': 'Read the latest record',
        u'设置RTU时间，输入%LOCALTIME%设置当前时间': 'Set the RTU time, enter %Localtime% to set the current time',
        u'RTU时间': 'RTU time',
        u'清空RTU存储数据': 'Clear RTU all stored data',
        u'置高或置低输出管脚': 'Set or Reset LOGIC output pin',
        u'置高或置低': 'Set or Reset',
        u': 置高': ': Set',
        u': 置低': ': Reset',
        u'AD管脚校准信息': 'AD pin calibration information',
        u'斜率': 'Slope',
        u'偏移': 'Deviation',
        u'阻值': 'Resistance',
        u'上传服务器的数据是否需要响应': 'Whether response is required for uploading data to the server',
        u'是否响应': 'Required',
        u'RTU报文格式': 'RTU uploading packet format',
        u'报文格式': 'Format',
        u': 字符串格式': ': String',
        u': ID+字符串格式': ': ID+String',
        u'4G模块APN设置': 'Mobile module the access point name configuration',
        u'协议类型': 'Internet protocol',
        u': 忽略': ': Ignore',
        u'认证类型': 'Authentication',
        u'NB模块休眠延时': 'Delay before NB module sleep',
        u'RTU重启': 'RTU reboot',
        u'RTU休眠延时': 'Delay before RTU sleep',
        u'服务器类型': 'Server type',
        u': 主服务器': ': Main server',
        u': MQTT服务器': ': MQTT server',
        u'设备地址': 'ID',
        u'功能码': 'Command',
        u'起始地址': 'Address',
        u'数据长度': 'Count',

        # products\product_rtu716\product.conf

        u'WRC716W-2AI设置': 'WRC716W-2AI',
        u'WRC-716W-2AI设置': 'WRC-716W-2AI',
        u'RTU主配置': 'RTU configuration',
        u'RTU MODBUS配置': 'MODBUS device configuration',
        u'RTU测试指令': 'RTU test AT command',
        u'RTU测试': 'RTU test AT command',

        # products\product_rtu716-2DI\at_description.conf


        # products\product_rtu716-2DI\product.conf

        u'WRC716W-2DI设置': 'WRC716W-2DI',
        u'WRC-716W-2DI设置': 'WRC-716W-2DI',

        # products\product_rtu816\at_description.conf

        u': 计数管脚': ': Plus count pin',
        u': 计速管脚': ': Plus speed pin',
        u': 计数超数报警': ': Over count alarm',
        u': 超速报警': ': Overspeed alarm',
        u': 低速报警': ': Underspeed alarm',
        u': 超速或低速都报警': 'Overspeed or underspeed alarm',
        u'计数初值': 'Count Initial',
        u'计数触发条件': 'Count trigger',
        u': 上升沿触发': ': Rising edge',
        u': 下降沿触发': ': Falling edge',
        u': 双沿触发': ': Edge trigger',
        u'计数报警': 'Count alarm',
        u'计速倍数': 'Count multiple',
        u'外部MODBUS设备读取指令1': 'MODBUS device read instruction 1',
        u'COMWAY报文协议下，COMWAY格式GPS数据上传配置': 'Upload GPS data by main server COMWAY Packet format',
        u'是否上传': 'Enable',
        u'保存RTU配置': 'Save RTU configuration',
        u'RTU复位': 'RTU reboot',
        u'RTU版本': 'RTU version',
        u'保存RTU校准信息': 'Save RTU calibration configuration',
        u'保存RTU短信报警配置': 'Save RTU SMS alarm configuration',
        u': 过压': ': Overvoltage',
        u': 欠压': ': Undervoltage',
        u': 高电位': ': High level',
        u': 低电位': ': Low level',
        u': 过量': ': Over count',
        u': 超速': ': Overspeed',
        u': 低速': ': Underspeed',
        u': 解除': ': Disarm',
        u'外部MODBUS设备没有响应的时候是否上传上一次的记录': 'Upload last record when MODBUS device is not responding',
        u'保存RTU扩展配置': 'Save RTU extend configuration',
        u'外部MODBUS设备读取指令2': 'MODBUS device read instruction 2',
        u'是否上传+CREG的信息': 'Upload +CREG response string',
        u'RTU报文协议': 'RTU data uploaded mode',
        u'报文协议': 'Upload mode',
        u': 主服务器决定': ': Main server packet format',
        u': 宏电协议': ': HONGDIAN packet format',
        u': HTTP协议': ': HTTP protocol',
        u': MQTT字符串协议': ': MQTT string format',
        u': MQTT CJSON协议': ': MQTT CJSON format',
        u': MQTT协议': ': MQTT protocol',
        u'RTU数据上传HTTP协议配置': 'Upload RTU data by HTTP protocol',
        u'RTU图片上传HTTP协议配置': 'Upload picture by HTTP protocol',
        u'获取摄像头参数': 'Get USBcam parameter',
        u'拍照并上传': 'Take picture and upload',
        u'分辨率': 'Resolution',
        u'文件名': 'File name',
        u'RTU上报数据格式和本机MODBUS地址': 'RTU Upload frame and local MODBUS address',
        u'数据格式': 'Frame format',
        u': MODBUS指令格式': ': MODBUS RTU',
        u': 不上传数据，只短信报警': ': No data mode, just SMS alarm',

        # products\product_rtu816\product.conf

        u'WRC816-2AI设置': 'WRC816-2AI',
        u'WRC-816-2AI设置': 'WRC-816-2AI',
        u'WRC-816设置': 'WRC-816',
        u'RTU短信报警配置': 'RTU SMS alarm configuration',
        u'RTU HTTP配置': 'RTU HTTP configuration',
        u'RTU MQTT配置': 'RTU MQTT configuration',

        # products\product_rtu826\at_description.conf


        # products\product_rtu826\product.conf

        u'WRC826设置': 'WRC826',
        u'WRC-826设置': 'WRC-826',

        # -----------------------------------------------------------------------------------------------

        # product_netviews\at_description.conf

        u'获取DTU错误记录，只2G DTU支持': 'Get DTU error records, only 2G DTU supported',
        u'错误记录': 'Error records',
        u'错误类型': 'Type',
        u': 无错误': ': No error',
        u': 限制服务': ': Limited service',
        u': 信号弱': ': Weak signal',
        u': sim卡读写错误': ': SIM card access error',
        u': 串口数据错误': ': Uart data error',
        u': 读临时文件错误': ': Read temporary file error',
        u': 写临时文件错误': ': Write temporary file error',
        u': 打开临时文件错误': ': Open temporary file error',
        u'月日时分': 'mdHM',
        u'清除DTU错误记录，只2G DTU支持': 'Clear DTU error records, only 2G DTU supported',
        u'获取串口状态': 'Get UART status',
        u'接收计数': 'Received count',
        u'发送计数': 'Sent count',
        u'BI错误计数': 'BI error count',
        u'FE错误计数': 'FE error count',
        u'PE错误计数': 'PE error count',
        u'OE错误计数': 'OE error count',
        u'清空串口状态': 'Clear UART status',
        u'获取服务器连接状态': 'Get server connection status',
        u'当前连接状态': 'Current status',
        u': 关闭连接': ': Connection closed',
        u': 正在连接': ': Connecting',
        u': 连接成功': ': Connect success',
        u'最后断链原因': 'Last error reason',
        u': dns错误': ': Dns error',
        u': dns超时': ': Dns timeout',
        u': 连接错误': ': Connect error',
        u': 连接超时': ': Connect timeout',
        u': 被服务器关闭': ': Connection closed by server',
        u': 空闲超时': ': Idle timeout',
        u': 发送错误': ': Send error',
        u': 无服务': ': No service',
        u': AT关闭连接': ': Connection closed by AT command',
        u'连接成功计数': 'Connect success',
        u'dns错误计数': 'Dns error',
        u'dns超时计数': 'Dns timeout',
        u'连接错误计数': 'Connect error',
        u'连接超时计数': 'Connect timeout',
        u'被关闭计数': 'Closed by server',
        u'空闲超时计数': 'Idle timeout',
        u'发送错误计数': 'Send error',
        u'无服务断链': 'No service',
        u'AT关闭连接': 'closed by AT',
        u'清空服务器连接状态': 'Clear server connection status',
        u'获取DTU重启记录，只2G DTU支持': 'Get DTU reboot records, only 2G DTU supported',
        u'重启记录': 'Reboot records',
        u'重启原因': 'Reason',
        u': AT指令重启': ': Reboot by AT command',
        u': 连接服务器失败次数超过10次重启': ': Failed to connect to the server more than 10 times',
        u': 无信号重启': ': No service',
        u': 无服务情况下定时重启': ': Scheduled Reboot when no service',
        u': 正常定时重启': ': Scheduled Reboot',
        u': 向服务器发送数据超时重启': ': Send timeout',
        u': 创建socket无内存重启': ': Out of memory',
        u': 创建socket失败重启': ': Create socket error',
        u'清空DTU重启记录': 'Clear DTU reboot records',
        u'查询信号强度': 'Query signal strength',
        u'信号强度': 'Signal strength',
        u'误码率': 'Error rate',
        u'发送短信': 'Send SMS',
        u'短信内容': 'SMS contents',
        u'RTU重启': 'RTU reboot',
        u'水文RTU重启': 'WRC820 reboot',
        u'IMEI号': 'IMEI number',
        u'PING主机': 'Ping host',
        u'主机': 'Host',

        # product_netviews\product.conf

        u'4G DTU 网管配置': '4G DTU Netviews',
        u'DTU状态信息': 'DTU status',

        # product_netviews2g\at_description.conf

        u'获取DTU错误记录': 'Get DTU error records',
        u'清除DTU错误记录': 'Clear DTU error records',
        u'获取DTU重启记录': 'Get DTU reboot records',

        # product_netviews2g\product.conf

        u'2G DTU 网管配置': '2G DTU Netviews',

        # -----------------------------------------------------------------------------------------------

        # products\product_dtu_main\product.conf

        u'DTU 主要配置': 'DTU main configuration',
        u'WL-4032 主要配置': 'WL-4032 DTU main configuration',

        # products\product_dtu_main\at_description.conf

        u'定时重启': 'Scheduled',
        u' 分钟 从0点开始': ' minutes Starting from 0 o\'clock',

        # products\product_dtu4G_mqtt_dual_topic\product.conf

        u'DTU-MQTT-多主题': 'DTU-MQTT',
        u'WL-4032-MQTT-多主题': 'WL-4032 DTU-MQTT',
        u'MQTT通信配置': 'MQTT communication configuration',
        u'MQTT透传配置': 'MQTT transparent configuration',
        u'MQTT采集配置': 'MQTT collection configuration',
        u'采集配置': 'Collection configuration',
        u'MQTT主题配置': 'MQTT topic configuration',
        u'串口通讯服务器配置': 'Socket & serial setting',
        u'GPS配置': 'GPS setting',
        u'HTTP通信配置': 'HTTP communication configuration',

        # products\product_dtu4G_mqtt_dual_topic\at_description.conf

        u': MQTT透传模式': ': MQTT transparent mode',
        u': MQTT采集模式': ': MQTT collection mode',
        u': 采集模式': ': Collection mode',
        u'MQTT串口发布主题': 'MQTT publish topic of COM transparent',
        u'MQTT串口订阅主题': 'MQTT subscribe topic of COM transparent',
        u'MQTT网口发布主题': 'MQTT publish topic of LAN transparent',
        u'MQTT网口订阅主题': 'MQTT subscribe topic of LAN transparent',
        u': AT+IPIDCONF指令索引0的发布主题': ': Publish topic set by AT+IPIDCONF 0',
        u': AT+IPIDCONF指令索引1的发布主题': ': Publish topic set by AT+IPIDCONF 1',
        u': AT+IPIDCONF指令索引2的发布主题': ': Publish topic set by AT+IPIDCONF 2',
        u': AT+IPIDCONF指令索引3的发布主题': ': Publish topic set by AT+IPIDCONF 3',
        u': AT+IPIDCONF指令索引4的发布主题': ': Publish topic set by AT+IPIDCONF 4',
        u': AT+IPIDCONF指令索引5的发布主题': ': Publish topic set by AT+IPIDCONF 5',
        u': AT+IPIDCONF指令索引6的发布主题': ': Publish topic set by AT+IPIDCONF 6',
        u': AT+IPIDCONF指令索引7的发布主题': ': Publish topic set by AT+IPIDCONF 7',

        u': AT+IPIDCONF指令索引0的订阅主题': ': Subscribe topic set by AT+IPIDCONF 0',
        u': AT+IPIDCONF指令索引1的订阅主题': ': Subscribe topic set by AT+IPIDCONF 1',
        u': AT+IPIDCONF指令索引2的订阅主题': ': Subscribe topic set by AT+IPIDCONF 2',
        u': AT+IPIDCONF指令索引3的订阅主题': ': Subscribe topic set by AT+IPIDCONF 3',
        u': AT+IPIDCONF指令索引4的订阅主题': ': Subscribe topic set by AT+IPIDCONF 4',
        u': AT+IPIDCONF指令索引5的订阅主题': ': Subscribe topic set by AT+IPIDCONF 5',
        u': AT+IPIDCONF指令索引6的订阅主题': ': Subscribe topic set by AT+IPIDCONF 6',
        u': AT+IPIDCONF指令索引7的订阅主题': ': Subscribe topic set by AT+IPIDCONF 7',

        u'RTU2TCP发布主题': 'MQTT publish topic of RTU2TCP',
        u'RTU2TCP订阅主题': 'MQTT subscribe topic of RTU2TCP',
        u'DTU采样参数': 'DTU sampling setting',
        u'MQTT定时采集发布主题': 'MQTT publish topic of sampling',
        u'采集指令设置': 'Sampling instruction setting',
        u': modbus指令': ': MODBUS instruction',
        u': 自定义hex指令': ': Custom instruction',
        u'指令类型': 'Type',
        u'服务器选择': 'Upload server',
        u': 采集数据通过串口服务器上传': ': Transparent server',
        u': 采集数据通过mqtt服务器上传(json格式)': ': MQTT broker(json format)',
        u': 采集数据通过mqtt服务器上传': ': MQTT broker',
        u': 采集数据通过HTTP服务器上传(json格式)': 'HTTP server(json format)',
        u'启用或关闭GPS': 'GPS switch',
        u': 停用': ': OFF',
        u': 启用': ': ON',
        u'MQTT_GPS数据发布主题': 'MQTT publish topic of GPS',
        u': 字符串': ': String',
        u': ID+字符串': ': ID+String',

        # products\product_dtu_main\product.conf

        u'WRC-816-PS设置': 'WRC-816-PS configuration',

        # products\product_qy_rtu816\at_description.conf

        u'HTTP请求链接': 'HTTP request url',
        u'请求链接': 'Request url',
        u'主题': 'Topic',
        u'MODBUS响应主题': 'MODBUS response topic',
        u'MODBUS指令主题': 'MODBUS instruction topic',
        u'AT响应主题': 'AT response topic',
        u'AT指令主题': 'AT instruction topic',

        # -----------------------------------------------------------------------------------------------

        # product_series_define.py

        u'支持WL-4010/4011/4030/4031/4050和4015/4055 ETHERNET DTU': 'Suport WL-4010/4011/4030/4031/4050 and 4015/4055 ETHERNET DTU',
        u'定制产品': 'Customized products',
        u'其它产品': 'Other products',
        u'设置socket通信、VPN通信参数&串口、网口参数': 'Socket, VPN, COM or ETHERNET communication setting',
        u'DI变化触发上传报文或短信报警': 'DI change triggers upload packet or SMS alarm',
        u'MODBUS RTU2TCP协议转换': 'Convert MODBUS RTU instruction to MODBUS TCP instruction',
        u'MODBUS TCP2RTU协议转换': 'Convert MODBUS TCP instruction to MODBUS RTU instruction',
        u'设置GPS定位信息采集和上传方式': 'GPS info upload mode setting',
        u'设置拍照和图片上传参数': 'Capture and upload picture setting',
        u'NBIOT RTU 全功能': 'NBIOT RTU with full-featured',
        u'MODBUS设备采集短信报警': 'Collect MODBUS device value, SMS alarm value overrun',
        u'多主题MQTT协议数据转发和modbus设备数据采集': 'MQTT protocol data forwarding and MODBUS device data collection',
        u'设置WL-4032 DTU的socket通信和串口参数': 'WL-4032 DTU Socket or COM communication setting',
        u'设置WL-4032 DTU的多主题MQTT协议数据转发和modbus设备数据采集': 'WL-4032 MQTT protocol data forwarding and MODBUS device data collection',
    }
}
